{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Arkusz1"],"read":"whole","date_system":"1900"}

{"sheet":"Arkusz1","index":0,"n_rows":49,"n_cols":30,"rows_kept":49,"merged":[[11,1,11,14],[11,16,11,29],[22,1,22,14],[22,16,22,29],[23,1,23,14],[23,16,23,29],[29,1,29,14],[29,16,29,29],[34,1,34,14],[34,16,34,29],[37,1,37,14],[37,16,37,29],[39,1,39,14],[39,16,39,29],[42,1,42,14],[42,16,42,29],[44,1,44,14],[44,16,44,29],[47,1,47,14],[47,16,47,29]]}
[]
[null,"UWAGA: ","pola wypełnione na żółto należy uzupełnić danymi tabelarycznymi z literatury (np. \"Wentylacja i klimatyzacja. Podstawy\" A. Pełech str.93-130)"]
[null,null,"pozostałe pola obliczane są wg odpowiednich wzorów"]
[null,null,"tabelę należy dostosować do własnego obiektu tzn. określić indywidualnie godziny jego pracy i zmodyfikować część związaną z przegrodami zewnętrznymi i kierunkami świata"]
[null,null,"w tabeli uwzględnia się tylko przegrody zewnętrzne (wewnętrzne są pomijane, chyba, że po dwóch stronach wewnętrznej przegrody występują istotne różnice w temperaturze pomieszczenia)"]
[]
[null,"LIPIEC",null,"tzśr =",null,"°C",{"$nulls":10},"WRZESIEŃ",null,"tzśr =",null,"°C"]
[]
[null,"Czas","jedn.",8,9,10,11,12,13,14,15,16,17,18,20,null,"Czas","jedn.",8,9,10,11,12,13,14,15,16,17,18,20]
[null,"tz","°C",{"$nulls":13},"tz","°C"]
[null,"tp","°C",{"$nulls":13},"tp","°C"]
[null,"Bilans ciepła przez przegrody nieprzezroczyste",{"$nulls":14},"Bilans ciepła przez przegrody nieprzezroczyste"]
[null,"Δtr (NE)","°C",{"$nulls":13},"Δtr (NE)","°C"]
[null,"Δtr' (NE)","°C",{"$nulls":13},"Δtr' (NE)","°C"]
[null,"Qpn (NE)","W",{"$nulls":13},"Qpn (NE)","W"]
[null,"Δtr (SE)","°C",{"$nulls":13},"Δtr (SE)","°C"]
[null,"Δtr' (SE)","°C",{"$nulls":13},"Δtr' (SE)","°C"]
[null,"Qpn (SE)","W",{"$nulls":13},"Qpn (SE)","W"]
[null,"Δtr (Std)","°C",{"$nulls":13},"Δtr (Std)","°C"]
[null,"Δtr' (Std)","°C",{"$nulls":13},"Δtr' (Std)","°C"]
[null,"Qpn (Std)","W",{"$nulls":13},"Qpn (Std)","W"]
[null,"Qpn","kW",{"$nulls":13},"Qpn","kW"]
[null,"Bilans ciepła przez przegrody przezroczyste",{"$nulls":14},"Bilans ciepła przez przegrody przezroczyste"]
[null,"Bilans ciepła przez promieniowanie",{"$nulls":14},"Bilans ciepła przez promieniowanie"]
[null,"Icmax (SE)","W/m2",{"$nulls":13},"Icmax (SE)","W/m2"]
[null,"Irmax (SE)","W/m2",{"$nulls":13},"Irmax (SE)","W/m2"]
[null,"s","-",{"$nulls":13},"s","-"]
[null,"b","-",{"$nulls":13},"b","-"]
[null,"Qr","W",{"$nulls":13},"Qr","W"]
[null,"Bilans ciepła przez przenikanie",{"$nulls":14},"Bilans ciepła przez przenikanie"]
[null,"U W/m2K","W/m2K",{"$nulls":13},"U W/m2K","W/m2K"]
[null,"Δt","°C",{"$nulls":13},"Δt","°C"]
[null,"Qp","W",{"$nulls":13},"Qp","W"]
[null,"Qpp","kW",{"$nulls":13},"Qpp","kW"]
[null,"Zyski ciepła jawnego od ludzi",{"$nulls":14},"Zyski ciepła jawnego od ludzi"]
[null,"qj","W/os",{"$nulls":13},"qj","W/os"]
[null,"QjL","kW",{"$nulls":13},"QjL","kW"]
[null,"Zyski ciepła jawnego od technologii",{"$nulls":14},"Zyski ciepła jawnego od technologii"]
[null,"QT","kW",{"$nulls":13},"QT","kW",0,null,{"$f":"S39","v":0},{"$f":"U39","v":0},{"$f":"V39","v":0},{"$f":"W39","v":0},{"$f":"X39","v":0},{"$f":"Y39","v":0},{"$f":"Z39","v":0},{"$f":"AA39","v":0},{"$f":"AB39","v":0},{"$f":"AC39","v":0}]
[null,"Zyski ciepła od oświetlenia",{"$nulls":14},"Zyski ciepła od oświetlenia"]
[null,"ko","-",{"$nulls":13},"ko","-"]
[null,"Qosw","kW",{"$nulls":13},"Qosw","kW"]
[null,"BILANS CIEPŁA JAWNEGO W LIPCU",{"$nulls":14},"BILANS CIEPŁA JAWNEGO WE WRZEŚNIU"]
[null,"Qzbj(oc)","kW",{"$nulls":13},"Qzbj(oc)","kW"]
[null,"Zyski ciepła całkowitego od ludzi",{"$nulls":14},"Zyski ciepła całkowitego od ludzi"]
[null,"qc","W/os",{"$nulls":13},"qc","W/os"]
[null,"QcL","kW",{"$nulls":13},"QcL","kW"]
[null,"BILANS CIEPŁA CAŁKOWITEGO W LIPCU",{"$nulls":14},"BILANS CIEPŁA CAŁKOWITEGO WE WRZEŚNIU"]
[null,"Qzbj(oc)","kW",{"$nulls":13},"Qzbj(oc)","kW"]