{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":445,"n_cols":6,"rows_kept":445,"flags":["formulas_cached_only"]}
[]
[null,"Strona","Kolumna","Oznaczenie","Urządzenie","Typ"]
[null," 2  "," 0  "," 2Q1  "," Rozłacznik 4G Apator  "," 4G63A  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 0  "," 2Q1  "," Rozłacznik  "," 4G25A  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 4  "," 1  "," 4F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 10  "," 4  "," 10Q1  "," Przełacznik 3-poz.  "," XB7-ED33P  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 4  "," 2G4  "," Grzałka elektryczna (opcja)  "," 500W 230V  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 7  "," 5  "," 7K2  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 9  "," 4  "," 9H2  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 10  "," 4  "," 10R1  "," Rezystor  "," 510om  "]
[null," 10  "," 4  "," 10R2  "," Rezystor  "," 510om  "]
[null," 11  "," 7  "," 11K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 11  "," 7  "," 11K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3P  "," XB7-ED33P  "]
[null," 12  "," 4  "," 12R1  "," Rezystor  "," 510om  "]
[null," 12  "," 4  "," 12R2  "," Rezystor  "," 510om  "]
[null," 13  "," 3  "," 13K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 7  "," 5  "," 7K2  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 9  "," 4  "," 9H2  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 10  "," 4  "," 10R1  "," Rezystor  "," 510om  "]
[null," 10  "," 4  "," 10R2  "," Rezystor  "," 510om  "]
[null," 11  "," 7  "," 11K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 11  "," 7  "," 11K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3P  "," XB7-ED33P  "]
[null," 12  "," 4  "," 12R1  "," Rezystor  "," 510om  "]
[null," 12  "," 4  "," 12R2  "," Rezystor  "," 510om  "]
[null," 13  "," 3  "," 13K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 0  "," 2Q1  "," Rozłacznik  "," 4G25A  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 4  "," 1  "," 4F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 10  "," 4  "," 10Q1  "," Przełacznik 3-poz.  "," XB7-ED33P  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 4  "," 2G4  "," Grzałka elektryczna (opcja)  "," 500W 230V  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 7  "," 5  "," 7K2  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 9  "," 4  "," 9H2  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 10  "," 4  "," 10R1  "," Rezystor  "," 510om  "]
[null," 10  "," 4  "," 10R2  "," Rezystor  "," 510om  "]
[null," 11  "," 7  "," 11K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 11  "," 7  "," 11K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3P  "," XB7-ED33P  "]
[null," 12  "," 4  "," 12R1  "," Rezystor  "," 510om  "]
[null," 12  "," 4  "," 12R2  "," Rezystor  "," 510om  "]
[null," 13  "," 3  "," 13K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV- "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 5  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3-poz..  "," XB7-ED33P  "]
[null," 13  "," 3  "," 13K1  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 2  "," 8K2  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 0  "," 2Q1  "," Rozłacznik  "," 4G25A  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," 80VA transformator  "," TR 220/24V  "]
[null," 3  "," 1  "," 3F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 4  "," 1  "," 4F1  "," Zabezpieczenie instalacyjne  "," S303 C10  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 7  "," 3  "," 7K1  "," 24VAC przekaznik pomocniczy  "," Finder5534  "]
[null," 7  "," 5  "," 7K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," \u0004ółta lampka sygnalizacyjna  "," ZBV-B5  "]
[null," 9  "," 4  "," 9H2  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," zielona lampka sygnalizacyjna  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," czerwona lampka sygnalizacyjna  "," ZBV-B4  "]
[null," 10  "," 4  "," 10Q1  "," Przełacznik 3-poz.  "," XB7-ED33P  "]
[null," 11  "," 7  "," 11K2  "," 24VAC przekaznik pomocniczy  "," Finder 5534  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 5  "," 1  "," 5K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 7  "," 1  "," 7K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 8  "," 1  "," 8K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 11  "," 7  "," 11K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 4  "," 2G4  "," Grzałka elektryczna (opcja)  "," 500W 230V  "]
[null," 2  "," 5  "," 2T2  "," Termostat (opcja)  "," RTR 3521  "]
[null," 2  "," 7  "," 2F1  "," Zabezpieczenie instalacyjne  "," S301 B6  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 35A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]
[null," 7  "," 3  "," 7K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 7  "," 5  "," 7K2  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 8  "," 1  "," 8H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 8  "," 5  "," 8H2  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 1  "," 9H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 9  "," 3  "," 9K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 9  "," 4  "," 9H2  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 5  "," 9H3  "," Lampka sterownicza zielona  "," ZBV-B3  "]
[null," 9  "," 6  "," 9H4  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 9  "," 8  "," 9H5  "," Lampka sterownicza czerwona  "," ZBV-B4  "]
[null," 10  "," 4  "," 10R1  "," Rezystor  "," 510om  "]
[null," 10  "," 4  "," 10R2  "," Rezystor  "," 510om  "]
[null," 11  "," 7  "," 11K1  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 11  "," 7  "," 11K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 12  "," 2  "," 12Q1  "," Przełacznik 3P  "," XB7-ED33P  "]
[null," 12  "," 4  "," 12R1  "," Rezystor  "," 510om  "]
[null," 12  "," 4  "," 12R2  "," Rezystor  "," 510om  "]
[null," 13  "," 3  "," 13K1  "," Przekaznik pomocniczy 24VAC  "," Finder 5534  "]
[null," 13  "," 4  "," 13K2  "," Przekaznik pomocniczy 24VAC  "," Finder 4052  "]
[null," 3  "," 1  "," 3K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 4  "," 1  "," 4K1  "," 24VAC przekaznik pomocniczy  "," F4052  "]
[null," 2  "," 8  "," 2F2  "," Zabezpieczenie instalacyjne  "," S301 C3  "]
[null," 2  "," 8  "," 2H1  "," Lampka sterownicza \u0004ółta  "," ZBV-B5  "]
[null," 2  "," 8  "," 2T1  "," Transformator 80VA  "," TR 220/24V  "]
[null," 3  "," 1  "," 3Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 4  "," 1  "," 4Q1  "," Rozłacznik bezpiecznikowy  "," R303 25A  "]
[null," 5  "," 1  "," 5F1  "," Zabezpieczenie instalacyjne  "," S301 C6  "]
[null," 5  "," 3  "," 5F2  "," Zabezpieczenie instalacyjne  "," S301 C10  "]